### Introduction

This document is designed as a reference and description of the various features of AU Lab 2.2. The Table of Contents in the left frame may be used to quickly jump to various sections of interest. Additionally, links within each section provide cross references to related information.

The top of each section contains a summary that briefly describes the contents and important points of the page:

Summary: A summary text block looks like this. You can scan the summary to determine if you are interested in topics contained on that specific page.

This document is best viewed in a web browser such as Safari that supports css.

#### What is AU Lab?

AU Lab is a digital mixing application that provides facilities for blending audio from the input of an audio device as well as audio generated by an Audio Unit Instrument or Generator. In addition, AU Lab can host Audio Unit effects and route audio through these effects.

The AU Lab Application

AU Lab is very efficient and has a very high performance and low overhead audio engine capable of supporting multiple outputs, full support for multichannel, and advanced routing features such as send buses and sidechain buses.

As the image above illustrates, the application provides MIDI clock facilities for audio units that support host clock synchronization, and an inspector that features a cocoa-based generic view of audio units that do not provide their own custom user interface. This inspector includes full support for preset management, and facilities for MIDI mapping of audio unit parameters.

Although AU Lab provides recording controls, it is not designed to be used for extensive recording. It is mainly designed as a platform reference Audio Unit host, and is designed for Audio Unit auditioning and live applications.

#### New Features in AU Lab

New features include:

- New document configuration editor
- Automatic creation of aggregate devices
- Improved document configuration management